# Test case with multiple z stepper motors
CONFIG multi_z.cfg
DICTIONARY atmega2560-16mhz.dict

# Start by homing the printer.
G28
G1 F6000

# Z / X / Y moves
G1 Z1
G1 X1
G1 Y1

# Run bed_tilt_calibrate
BED_TILT_CALIBRATE

# Move again
G1 Z5 X0 Y0

# Run Z_TILT_ADJUST
Z_TILT_ADJUST

# Move again
G1 Z2 X2 Y3

# Do regular probe
PROBE
QUERY_PROBE

# Verify stepper_buzz
STEPPER_BUZZ STEPPER=stepper_z
STEPPER_BUZZ STEPPER=stepper_z1
STEPPER_BUZZ STEPPER=stepper_z2

# Move again
G1 Z9
